**Jake’s Shoes - Notes**

**Class 1 - Team Gas Forging Specimens (Saturday - 1 ½ hours)**

¾ Fullered Calkin and Wedge

Toe to outside heel = 5” ½

Toe to inside heel = 5”

Width = 4” ¾

Nail - E4 Slim

Made from 12” of 3/8 x ¾

Aluminium Straight Bar Shoe

Length = 5” 9/16

Width = 5” ½

Bar = 3” 3/8

Nail - E4 Slim

Made from 15” of 3/8 x 1

Toe piece made from ¼” round steel

**Class 2 - (Shoeing) Specimens (Saturday - 2 hours)**

Workhorse Front Shoe

Centre of toe to outside = 6” 7/8

Centre of toe to inside = 6” 3/4

Width = 6” 3/16

Nail - E7 Slim

Made from 16" of ½ x 1

Bar made from 5/8 square

Hackney Bar Shoe

Width = 4” 5/8

Length, toe to heels = 6” ¼

Nail - 6 City Slim

Made from 12 ½ inches of 3/8 x 1"

**Class 3 - (Shoeing) Specimens (Sunday - 1 ½ hours)**

Fully Fullered/Deep Seated Front Bar Shoe

Length 6 1/2

Width 6 3/8"

Bar 3 3/4"

Nail - E7 Slim

Made from 16" of 1/2x 1"

Hammer finished

European Bar Shoe

Length 5” ½

Width 5” 1/16

Bar 2” 7/8

Nail - E4 Slim

Made from 14 ½” of 3/8 x 1”